For 1990-2009 cars
Automatic Transmission Components
Automatic Transmission Controls Schematics
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The brake switch indicates brake pedal status to the Powertrain Control Module (PCM). The brake switch is a normally-closed switch that supplies battery voltage on circuit 420 to the PCM. Applying the brake pedal opens the switch, interrupting voltage to the PCM. When the brake pedal is released, the PCM receives a constant voltage signal. If the PCM receives a zero voltage signal at the brake switch input, and the Torque Converter Clutch (TCC) is engaged, the PCM de-energizes the Torque Converter Clutch Solenoid Valve (TCC Sol. Valve).

When the PCM detects a closed brake switch (pedal released) during a number of decelerations, then DTC P0724 sets. DTC P0724 is a type D DTC.

### Conditions for Setting the DTC

• | No VSS DTCs P0502 or P0503.

• | The vehicle speed is greater than 32 km/h (20 mph) for more than 6 seconds.

• | The vehicle speed decreases to 8 km/h (5 mph) and takes more than 4 seconds.

• | The vehicle speed is less than 8 km/h (5 mph).

• | The above conditions must occur more than 7 times with the brake switch continuously closed, (PCM receiving voltage), without being open for more than 2 seconds.

### Action Taken When the DTC Sets

The PCM does not illuminate the Malfunction Indicator Lamp (MIL).

### Conditions for Clearing the DTC

A scan tool can clear the DTC from the PCM history. The PCM clears the DTC from the PCM history if the vehicle completes 40 warm-up cycles without a failure reported.

### Diagnostic Aids

• | Ensure that the brake switch is properly adjusted.

• | Inspect the wiring at the PCM, the brake switch connector and all other circuit connecting points for the following conditions:

- | A bent terminal

- | A backed out terminal

- | A damaged terminal

- | Poor terminal tension

- | A chafed wire

- | A broken wire inside the insulation

- | Moisture intrusion

- | Corrosion

• | When diagnosing for an intermittent short or open condition, massage the wiring harness while watching the test equipment for a change.

### Test Description

The number below refers to the step numbers on the diagnostic table.

1. A Scan Tool display that changes from Closed to Open when the brake switch is disconnected indicates a faulty brake switch.

#### DTC P0724 TCC Brake Switch Circuit High

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Powertrain On-Board Diagnostic (OBD) System Check performed? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check in Engine Controls
2 |

1. Install the Scan Tool .
2. With the engine OFF, turn the ignition switch to the RUN position.

Important: Before clearing the DTCs, use the Scan Tool in order to record the Freeze Frame and Failure Records for reference. Using the Clear Info function will erase the stored Freeze Frame and Failure Records from the PCM.

3. Record the DTC Failure Records, then clear the DTC.
4. Select Brake Switch on the Scan Tool .
5. Disconnect the brake switch connector.

Did the brake switch status change from Closed to Open?

--

Go to Step 3

Go to Step 4

3 | Adjust or replace the Brake Switch. Refer to Stoplamp Switch Adjustment or Stoplamp Switch Replacement in Hydraulic Brakes. Is the replacement complete? | -- | Go to Step 7 | --
4 | Inspect circuit 420 for a short to power. Repair circuit 420 if necessary. Refer to General Electrical Diagnosis Procedures in Wiring Systems. Was a condition found and corrected? | -- | Go to Step 7 | Go to Step 5
5 | Inspect circuits 420 and 1339 for a short together. Repair circuits 420 or 1339 if necessary. Refer to General Electrical Diagnosis Procedures in Wiring Systems. Was a condition found and corrected? | -- | Go to Step 7 | Go to Step 6
6 | Replace the PCM. Refer to Powertrain Control Module Replacement/Programming in Engine Controls. Is the replacement complete? | -- | Go to Step 7 | --
7 | In order to verify your repair, perform the following procedure:

1. Using the Scan Tool , clear DTC information.
2. Operate the vehicle under the following conditions:

• | Turn the ignition switch to the RUN position.

• | Apply the brake pedal. The Brake Switch must be open for more than 2 seconds.

3. Select Specific DTC. Enter DTC P0724.

Has the test run and passed?

--

System OK

Go to Step 1