For 1990-2009 cars

#### Tools Required

J 24086-C Piston Pin Remover/Installer

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

1. Disassemble the piston rings. Use a suitable tool in order to expand the rings. Do not re-use the piston rings.

Important: Make sure that no load is put on the piston during disassembly.

2. Place the piston and connecting rod assembly into the J 24086-C . Ensure that the flat side or the inside of the piston is up when installing the piston and rod assembly into the fork.
3. Press out the piston pin.