For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Wiper/Washer System Check performed? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Set the ignition switch to RUN.
2. Set the wiper switch to OFF.
3. Disconnect the wiper/washer switch connector C201.

Does the wiper keep running?

--

Go to Step 6

Go to Step 3

3 | Check for a short to voltage in the pigtail wires to the wiper/washer switch. Is a short to voltage present? | -- | Go to Step 5 | Go to Step 4
4 | Replace the wiper/washer switch. Refer to Multifunction, Turn Signal, and Hazard Switch Replacement - On Vehicle . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
5 | Repair the short to voltage in the pigtail wires to the wiper/washer switch. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Measure the voltage from connector C201 (vehicle side), terminal E2, to ground with a DMM. Is the measurement greater than the specified value? | 1.0 V | Go to Step 14 | Go to Step 7
7 | Measure the voltage from connector C201 (vehicle side), terminal E3, to ground with a DMM. Is the measurement greater than the specified value? | 1.0 V | Go to Step 11 | Go to Step 8
8 |

1. Reconnect the wiper/washer switch connector C201.
2. Disconnect the wiper motor connector.
3. Measure the voltage from wiper motor connector, terminal C, to ground with a DMM.

Is the measurement within the specified range?

10.5-15 V

Go to Step 9

Go to Step 10

9 | Repair the short to voltage in CKT 92. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
10 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
11 |

1. Reconnect the wiper/washer switch connector C201.
2. Disconnect the wiper motor connector.
3. Measure the voltage from wiper motor connector, terminal E, to ground with a DMM.

Is measurement greater than the specified value?

1.0 V

Go to Step 12

Go to Step 13

12 | Repair the short circuit to battery voltage condition in CKT 112. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
13 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
14 |

1. Reconnect the wiper/washer switch connector C201.
2. Disconnect the wiper motor connector.
3. Measure the voltage from wiper motor connector, terminal D, to ground with a DMM.

Is the measurement greater than the specified value?

1.0 V

Go to Step 16

Go to Step 15

15 | Replace the wiper motor cover. Refer to Wiper Motor Cover Replacement . Is the replacement complete? | -- | Go to Wiper/Washer System Check | --
16 | Repair the short to voltage in CKT 113. Is the repair complete? | -- | Go to Wiper/Washer System Check | --