For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Has the Park Brake System Check been performed? | -- | Go to Step 2 | Go to Park Brake System Check
2 | Inspect the park brake actuator levers at the end of the left rear and right rear park brake cables. Are both of the park brake actuator levers in their full release positions? | -- | Go to Step 3 | Go to Step 4
3 | Adjust the brake shoes. Refer to Drum Brake Adjustment in Drum Brakes. Has the inspection/repair been performed? | -- | Go to Step 5 | --
4 | Inspect the park brake cables for binding. Replace as necessary. Has the inspection/repair been performed? | -- | Go to Step 5 | --
5 |

1. Release the park brake.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle

Important: Slight brake lining drag is considered normal.

3. Use your hands in order to rotate the rear wheels.

Do the rear wheels rotate freely?

--

System OK

Go to Step 1