For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Outside Mirrors System Check performed? | -- | Go to Step 2 | Go to Outside Mirrors System Check
2 |

1. Set the mirror select switch to the LEFT or RIGHT position, as needed.
2. If the left mirror is inoperative, backprobe with a test lamp from the outside rearview mirror remote control switch connector terminal G to terminal H.
3. If the right mirror is inoperative, backprobe with a test lamp from the outside rearview mirror remote control switch connector terminal A to terminal C.
4. While observing the test lamp, press the mirror position switch to the UP position.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 |

1. Using a test lamp, backprobe from the inoperative outside rearview mirror connector terminal B to terminal C.
2. Press the mirror position switch to the UP position while observing the test lamp.

Does the test lamp light?

--

Go to Step 5

Go to Step 6

4 | Replace the outside rearview mirror remote control switch. Refer to Door Trim Plate Replacement . Is the repair complete? | -- | Go to Step 7 | --
5 | Replace the mirror motor pack within the power mirror. Refer to Outside Rearview Mirror Motor Replacement . Is the repair complete? | -- | Go to Step 7 | --
6 |

1. If the left mirror is inoperative repair the open in CKT 88.
2. If the right mirror is inoperative repair the open in CKT 1498.

Is the repair complete?

--

Go to Step 7

--

7 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors/components removed.

Have all the repairs been made?

--

Go to Outside Mirrors System Check

--