For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Bucket Seat Replacement .
2. Remove the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
3. Remove the seat back pad. Refer to Front Seat Back Cushion Pad Replacement .
4. Unhook the lateral release cables from the seat back frame (1) and the recliner.
5. Remove the lateral release assembly from the seat back frame (1).

### Installation Procedure

1. Install the lateral release assembly to the seat back frame (1).
2. Hook the lateral release cables to the seat back frame (1) and the recliner.
3. Install the seat back pad. Refer to Front Seat Back Cushion Pad Replacement .
4. Install the seat back cover. Refer to Front Seat Back Cushion Cover Replacement .
5. Install the front seat. Refer to Bucket Seat Replacement .