For 1990-2009 cars

### Removal Procedure

1. Remove the instrument upper trim panel. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gauges and Console.
2. Pull the side window defroster duct from the instrument panel.
3. Remove side window defroster duct from instrument panel.

### Installation Procedure

1. Position side window defroster duct to instrument panel.
2. Push the side window defroster duct to snap duct into the instrument panel.
3. Install the instrument upper trim panel. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gauges and Console.