For 1990-2009 cars

### Removal Procedure

1. Remove the front door outside handle. Refer to Front Side Door Outside Handle Replacement .
2. Remove the lock cylinder retainer from the front door outside handle.
3. Remove the front door lock cylinder from the front door outside handle.

### Installation Procedure

1. Install the front door lock cylinder to the front door outside handle.
2. Install the lock cylinder retainer to the front door outside handle.
3. Install the front door outside handle. Refer to Front Side Door Outside Handle Replacement .