For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Do the exterior turn lamps flash? | -- | Go to Step 2 | Go to Exterior Lights System Check in Lighting Systems
2 | Does the high beam indicator work with the high beams on? | -- | Go to Step 3 | Go to Instrument Cluster Illumination Lamps Inoperative
3 | Check for a poor connection or open in the following circuits:

• | (Left) CKT 18 between the instrument cluster harness connector C2 terminal P and S233.

• | (Right) CKT 19 between the instrument cluster harness connector C2 terminal R and S232.

Is there a poor connection or open.

--

Go to Step 4

Go to Step 5

4 | Repair the poor connection or open in the following circuits:

• | (Left) CKT 18 between the instrument cluster harness connector C2 terminal P and S233.

• | (Right) CKT 19 between the instrument cluster harness connector C2 terminal R and S232.

Has the repair been made and the system rechecked?

--

System OK

--

5 |

1. Check the warning indicator bulb and bulb connection.
2. If OK, replace the instrument cluster. Refer to Instrument Cluster Replacement .

Has the repair been made and the system rechecked?

--

System OK

--