For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the tilt lever. Refer to Tilt Lever Replacement - On Vehicle .
3. Remove the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle .
4. Remove the steering column trim covers. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .

### Installation Procedure

1. Install the steering column trim covers. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .
2. Install the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement - On Vehicle .
3. Install the tilt lever. Refer to Tilt Lever Replacement - On Vehicle .
4. Enable the SIR system. Refer to Enabling the SIR System in SIR.