For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Drain the engine oil.
3. Disconnect the electrical connector from Engine Oil Level Switch (1).
4. Remove the Engine Oil Level Switch from the oil pan.

### Installation Procedure

1. Install the Engine Oil Level Switch.
2. Connect the electrical connector to Engine Oil Level Switch (1).
3. Check and fill oil to proper level, refer to General Information