For 1990-2009 cars

### Removal Procedure

1. Grasp both sides of the quick-connect fitting. Twist the female connector 1/4 turn in each direction in order to loosen any dirt within the quick-connect fitting.

Caution: Wear safety glasses when using compressed air in order to prevent eye injury.

2. Using compressed air, blow any dirt out of the quick-connect fitting.
3. Squeeze the plastic retainer release tabs.
4. Pull the connection apart.

### Installation Procedure

Caution: In order to reduce the risk of fire and personal injury, before connecting fuel pipe fittings, always apply a few drops of clean engine oil to the male pipe ends.

This will ensure proper reconnection and prevent a possible fuel leak. During normal operation, the O-rings located in the female connector will swell and may prevent proper reconnection if not lubricated.

1. Apply a few drops of clean engine oil to the male fuel pipe end.
2. Push both sides of the quick-connect fitting together in order to cause the retaining tabs/fingers to snap into place.
3. Once installed, pull on both sides of the quick-connect fitting in order to make sure the connection is secure.