For 1990-2009 cars

## Fastener Tightening Specifications Unit Repair

#### Fastener Tightening Specifications

Part Number | Description of Use | Qty | Thread Size | Specifications
--- | --- | --- | --- | ---
Metric | English
5 | Bolt, Case Extension | 4 | M10 x 1.5 x 35.0 | 35.5 N·m | 26.0 lb ft
9 | Bolt, Speed Sensor | 1 | M8 x 1.25 x 12.0 | 11.0 N·m | 97.5 lb in
12 | Bolt, FWD Servo Cover | 3 | M6 x 1.0 x 20.0 | 10.0 N·m | 88.5 lb in
23 | Bolt, Oil Pan | 20 | M6 x 1.0 x 17.0 | 11.5 N·m | 95.0 lb in
28 | Ball Check Assembly, Cooler | 1 | 3/8-18 | 52.0 N·m | 38.5 lb ft
29 | Connector--Cooler (Inverted Flared Tube) | 1 | 1/4-18 | 38.0 N·m | 28.0 lb ft
30 | Bolt, Modulator | 1 | M8 x 1.25 x 20.0 | 23.5 N·m | 17.3 lb ft
38 | Plug, Pipe--(Line Pressure) | 2 | 1/8-27 | 10.5 N·m | 93.0 lb in
50 | Nut, Case Side Cover (Flanged Hex) | 6 | M6 x 1.0 | 8.0 N·m | 71.2 lb in
52 | Screw and Conical Washer Assembly | 17 | M8 x 1.25 x 21.3 | 11.0 N·m | 97.5 lb in
56 | Bolt, Metric Hex (Structural Side Cover) | 11 | M8 x 1.25 x 25.0 | 23.5 N·m | 17.3 lb ft
57 | Bolt, Torx® Head (Structural Side Cover) | 4 | M8 x 1.25 x 21.0 | 23.5 N·m | 17.3 lb ft
58 | Stud, Structural Side Cover to Case | 2 | M8 x 1.25 x 25.0 | 23.5 N·m | 17.3 lb ft
103 | Bolt, 2-1 Manual Servo Cover | 3 | M8 x 1.25 x 25.0 | 23.5 N·m | 17.3 lb ft
131 | Bolt, Hex Flange (Accumulator Cover and Housing) | 11 | M6 x 1.0 x 28.0 | 11.0 N·m | 97.5 lb in
204 | Bolt, Pump Cover to Valve Body | 1 | M6 x 1.0 x 45.0 | 11.0 N·m | 97.5 lb in
205 | Bolt, Pump Cover to Pump Body | 1 | M8 x 1.25 x 20.0 | 23.5 N·m | 17.3 lb ft
206 | Bolt, Pump Body to Case | 2 | M8 x 1.25 x 95.0 | 23.5 N·m | 17.3 lb ft
207 | Bolt, Pump Cover to Channel Plate | 9 | M6 x 1.0 x 85.0 | 11.0 N·m | 97.5 lb in
375 | Bolt, Valve Body to Case | 3 | M8 x 1.25 x 70.0 | 23.5 N·m | 17.3 lb ft
376 | Bolt, Valve Body to Channel Plate | 1 | M6 x 1.0 x 35.0 | 11.0 N·m | 97.5 lb in
377 | Bolt, Valve Body to Channel Plate (Torx®) | 2 | M6 x 1.0 x 45.0 | 12.0 N·m | 9.0 lb ft
378 | Bolt, Valve Body to Channel Plate | 6 | M6 x 1.0 x 55.0 | 11.0 N·m | 97.5 lb in
379 | Bolt, Special, Valve Body to Case | 1 | M8 x 1.25 x 85.0 | 23.5 N·m | 17.3 lb ft
380 | Bolt, Valve Body to Case | 1 | M8 x 1.25 x 90.0 | 23.5 N·m | 17.3 lb ft
434 | Bolt, Channel Plate to Case | 6 | M8 x 1.25 x 45.0 | 23.5 N·m | 17.3 lb ft
436 | Bolt, Channel Plate to Case | 4 | M8 x 1.25 x 30.0 | 23.5 N·m | 17.3 lb ft
450 | Temperature Sensor | 1 | 1/8-27 | 7.0 N·m | 62.0 lb in
524 | Screw, Case to Drive Sprocket Support | 4 | M8 x 1.25 x 23.5 | 23.5 N·m | 17.3 lb ft
803 | Nut, Manual Shaft to Detent Lever | 1 | M10 x 1.5 | 31.5 N·m | 23.2 lb ft
805 | Bolt, Special, Manual Detent Sprig to Channel Plate | 1 | M6 x 1.0 x 16.0 | 11.0 N·m | 97.5 lb in

## Fastener Tightening Specifications On-Vehicle

Application | N·m | Lb Ft | Lb In
--- | --- | --- | ---
Accumulator Bolt | 11 | -- | 97
Case Extension Housing Bolts | 36 | 27 | --
Case Side cover Nut | 8 | -- | 71
Case Side Cover Bolt | 11 | -- | 97
Converter Cover Bolt | 10 | -- | 89
Drivetrain and Front suspension Frame Bolts | 180 | 133 | --
Fluid Filler Tube Bolt | 13 | -- | 115
Fluid Filler Tube Nut | 13 | -- | 115
Flywheel to Torque Converter Bolt | 63 | 46 | --
Inside Detent Lever Nut | 32 | 24 | --
Manual Detent Roller Bolt | 11 | -- | 97
Oil Cooler Pipe to Transaxle | 23 | 17 | --
Oil Cooler Pipe to Radiator | 23 | 17 | --
Oil Cooler Hose Clamp | 2 |  | 18
Oil Pan Bolt | 11 | -- | 97
Pump M6 Bolts | 11 | -- | 97
Pump M8 Bolts | 24 | 18 | --
Servo Cover Bolt | 11 | -- | 97
Shift Cable Bracket Bolt | 27 | 20 | --
Transaxle Brace Bolts | 47 | 35 | --
Transaxle Front Mount Upper Nut | 44 | 32 | --
Transaxle Front Mount Lower Nuts | 44 | 32 | --
Front Transaxle Bracket Bolts | 55 | 41 | --
Rear Mount Upper Nut | 44 | 32 | --
Rear Mount Lower Nuts | 25 | 18 | --
Rear Transaxle Bracket Bolts | 55 | 41 | --
Transaxle to Engine Bolt | 75 | 55 | --
Transaxle Range Switch Bolt | 25 | 18 | --
Transaxle Range Switch Shift Lever Nut | 20 | 15 | --
Vacuum Modulator Clamp Bolt | 24 | 18 | --
Valve Body M6 Bolts | 11 | -- | 97
Valve Body M8 Bolts | 24 | 18 | --
Vehicle Speed Sensor Bolt | 11 | -- | 97