For 1990-2009 cars

1. Remove the upper and lower trim covers. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
2. Pop the wire harness assembly (4) out of the wire harness strap (5).
3. Remove the wire harness straps (3) from the wire harness assembly (4).
4. Remove 1 wire harness strap (2) from the upper tilt head assembly (1).
5. Slide the turn signal switch assembly connectors (2) out from the bulk head connector (1).
6. Remove the key alarm connector (1) from the lock module assembly (2).
7. Remove the 2 tapping screws from the ignition key alarm switch assembly (3).