For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Wheel Removal in Tires and Wheels.
3. Remove the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
4. Remove and DISCARD the wheel bearing/hub bolts.
5. Remove the wheel bearing/hub.
6. Remove the wheel speed sensor electrical connector (2).

### Installation Procedure

1. Install the wheel speed sensor electrical connector (2).
2. Install the wheel bearing/hub.

Notice: Refer to Fastener Notice in the Preface section.

Caution: These fasteners MUST be replaced with new fasteners anytime they become loose or are removed. Failure to replace these fasteners after they become loose or are removed may cause loss of vehicle control and personal injury.

3. Install the NEW wheel bearing/hub bolts.

Tighten
Tighten the NEW wheel bearing/hub bolts to 80 N·m (59 lb ft).

4. Install the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
5. Install the tire and wheel. Refer to Wheel Installation in Tires and Wheels.
6. Lower the vehicle.