For 1990-2009 cars

Important: Do not use any type of adhesive or sealer when assembling the gaskets. You may use Transjel™ or equivalent as an aid.

1. Assemble the upper and lower gaskets (430, 429) for the automatic transmission case cover.
2. Hold the manual valve in place and carefully assemble the case cover (400) onto the pins in the case.

Important: Do not use an impact wrench in order to tighten cover bolts.

3. Finger start all transmission case cover bolts into the locations noted (434, 436, 805).
4. Use 10 mm and 13 mm sockets in order to tighten all the bolts.

Tighten
Tighten all the bolts to 20.0-27.0 N·m (14.7-20.0 lb ft).

Refer to Fastener Notice .

5. Some transmission models have a temperature sensor (450) which is located in the case cover. Install the temperature sensor at this time.