For 1990-2009 cars

### Removal Procedure

1. Remove the left side instrument panel insulator. Refer to Instrument Panel Insulator in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connectors.
3. Remove the stoplamp switch (1) from the brake pedal bracket (2).

### Installation Procedure

1. Install the stoplamp switch (1) to the brake pedal bracket (2).
2. Connect the electrical connectors.
3. Install the left side instrument panel insulator. Refer to Instrument Panel Insulator in Instrument Panel, Gauges and Console.
4. Adjust the stoplamp switch. Refer to Stop Lamp Switch Adjustment .