For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | --
Heater-A/C Control | Center of the IP, below the radio | HVAC Component Views in HVAC Systems with A/C-Manual | HVAC Connector End Views in HVAC Systems with A/C-Manual
Rear Window Defogger Grid | Rear liftgate window | Stationary Windows Component Views | --
Rear Window Defogger Relay | Part of the relay center, right side of the IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control Systems | --
Relay Center | Right side of IP, mounted to the bracket along with the BCM, near the rear top right side of the IP compartment | Body Control System Component Views in Body Control Systems | Lighting Systems Connector End Views in Lighting Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G401 | Secured to the lower left D-pillar | Harness Routing Views in Wiring Systems | --
P406 | Between the right side of the liftgate and the roof | Harness Routing Views in Wiring Systems | --
S213 | IP harness, center of IP approximately 68 cm (27 in) from the cigar lighter | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S274 | IP harness, right side of the IP approximately 4 cm (2 in) from the BCM breakout | -- | --
S275 | IP harness, right side of the IP approximately 6 cm (2.5 in) from the BCM breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --