For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Stud Castle Nut (Lower Control Arm) | 55 N·m | 40 lb ft
Ball Stud Nuts (Replacement Ball Joint) * | 68 N·m | 50 lb ft
Lower Control Arm Nuts (at Frame) * | 113 N·m | 83 lb ft
Stabalizer Shaft Insulator Bracket Bolts | 48 N·m | 35 lb in
Stabilizer Shaft Link Nut | 23 N·m | 17 lb ft
Strut Lower Nuts (at Knuckle) * | 123 N·m | 90 lb ft
Strut Shaft Nut * | 85 N·m | 63 lb ft
Strut Upper Nuts | 41 N·m | 30 lb ft
Wheel Bearing/Hub Bolts (NEW ONLY) | 130 N·m | 96 lb ft
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.