For 1990-2009 cars

### Removal Procedure

1. Remove the body hinge pillar tie bar-cross car beam. Refer to Instrument Panel Tie Bar Replacement in Instrument Panel, Gauges and Console.
2. Release the snap tabs from the cross vehicle beam and remove the air distribution duct from the beam.

### Installation Procedure

1. Install the main air distribution duct into the cross vehicle beam.
2. Install the cross vehicle beam. Refer to Instrument Panel Tie Bar Replacement in Instrument Panel, Gauges and Console.