For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the outside rearview mirror nuts.
4. Disconnect the electrical connectors.
5. Remove the outside rearview mirror from the front door.

### Installation Procedure

1. Install the outside rearview mirror to the front door.
2. Connect the electrical connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the outside rearview mirror nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .