For 1990-2009 cars

#### Automatic Transaxle (C111)

Connector Part Information |

• | 12160493

• | 20-Way F Metri-Packard 100 W Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1222 | 1-2 shift solenoid valve control
B | YEL/BLK | 1223 | 2-3 shift solenoid valve control
C | RED/BLK | 1228 | Pressure control solenoid high
D | LT BLU/WHT | 1229 | Pressure control Solenoid low
E | PNK | 1339 | Fused ignition 1 feed
F-K |  |  | Not Used
L | YEL/BLK | 1227 | Transmission fluid temperature sensor signal
M | BLK | 2762 | Sensor ground
N | PNK | 1224 | Pressure switch A input
P | RED | 1226 | Pressure switch C input
R | DK BLU | 1225 | Pressure switch B input
S | RED/BLK | 1230 | Sensor ground
T | BRN | 418 | TCC PWM solenoid valve control
U | YEL | 657 | TCC Release switch input
V | DK BLU/WHT | 1231 | Sensor low
W |  |  | Not Used

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 812 | CMP sensor battery positive voltage (B+)
B | BLK | 630 | CMP sensor signal
C | BLK | 407 | CMP sensor ground

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12110293

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 1867 | CMP/CKP sensor ground
B | LT BLU/BLK | 647 | CKP sensor signal
C | YEL/BLK | 1868 | CMP/CKP sensor battery positive voltage

#### Engine Coolant Fan Motor 1 (RH)

Connector Part Information |

• | 12085030

• | 2-Way F Metri-Pack 630 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1050 | Ground
B | LT BLU | 409 | Engine coolant fan 1 (RH) feed

#### Engine Coolant Fan Motor 2 (RH)

Connector Part Information |

• | 12085030

• | 2-Way F Metri-Pack 630 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1050 | Ground
B | LT BLU | 409 | Engine coolant fan 2 (LH) feed

#### Engine Oil Level Indicator Switch

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1174 | Engine oil level indicator input
B | BLK/WHT | 451 | Ground

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (Red)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 339 | Fused ignition 1 feed
B | DK GRN/WHT | 428 | EVAP canister purge valve control

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (Red)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1039 | Fused ignition 1 feed
B | WHT | 1310 | Canister vent valve solenoid output

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 15324044

• | 5-way merti-pack 150 series (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | EGR solenoid output
B | BLK | 2753 | PCM Sensor ground
C | BRN | 1456 | EGR solenoid position signal
D | GRY | 2702 | 5-volt reference A
E | RED | 1676 | EGR valve coil feed

#### Fuel Pump Sender Unit C1

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1589 | Fuel level sensor input
B | GRY | 120 | Fuel pump motor feed
C | BLK | 250 | Ground
D | BLK/WHT | 2759 | Ground-clean

#### Fuel Tank Pressure Sensor C2

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 2759 | Ground-clean
B | DK GRN | 890 | Fuel tank pressure sensor signal
C | GRY/BLK | 2700 | 5-volt reference

#### Generator

Connector Part Information |

• | 12047950

• | 4-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A |  |  | Not Used
B | RED | 225 | Generator output-regulator reference voltage
C |  |  | Not Used
D |  |  | Not Used

#### Heated Oxygen Sensor 1 (HO2S 1)

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | HO2S 1 low
B | PPL | 412 | HO2S 1 signal
C | BLK | 1050 | Ground
D | PNK | 339 | Fused ignition 1 feed

#### Heated Oxygen Sensor 2 (HO2S 2)

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | HO2S 2 low
B | PPL/WHT | 1668 | HO2S 2 signal
C | BLK | 1050 | Ground
D | PNK | 339 | Fused ignition 1 feed

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | IAC motor feed-coil B low
B | LT GRN/WHT | 1749 | IAC motor feed-coil B high
C | LT BLU/BLK | 1748 | IAC motor feed-coil A low
D | LT BLU/WHT | 1747 | IAC motor feed-coil A high

#### Ignition Control Module (ICM) C1

Connector Part Information |

• | 12162260

• | 6-Way F Metri-Pack 150.2 Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 424 | Electronic spark timing bypass signal
B | WHT | 423 | Electronic spark timing control signal
C-D |  |  | Not Used
E | PPL/WHT | 430 | Electronic spark timing high reference signal
F | RED/BLK | 453 | Electronic spark timing low reference signal

#### Ignition Control Module (ICM) C2

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 51 | Ground-clean
B | PNK | 239 | Fused ignition 1 feed

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | IAT ground
B | TAN | 472 | IAT sensor input

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | MAF sensor input
B | BLK/WHT | 451 | Ground
C | PNK | 339 | Ignition 1 feed

#### Power Control Module (PCM) C1

Connector Part Information |

• | 12191110

• | 80-Way F Metri-Pack 100 W Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BLK | 2762 | Sensor ground
2 |  |  | Not Used
3 | ORN | 55 | Fuel level output
4 | LT GRN | 1222 | 1-2 shift solenoid valve control
5 | DK BLU | 473 | Fan 2 control (high speed)
6 | DK GRN | 335 | Fan 1 control (low speed)
7 | BLK | 630 | Camshaft position PCM input
8 | PPL/WHT | 430 | 3X reference
9 | LT BLU/BLK | 647 | 24X reference
10 | GRY | 2704 | 5 volt reference
11 |  |  | Not Used
12 | BLK | 2761 | ECT ground
13 | ORN/BLK | 469 | Map sensor ground
14 |  |  | Not Used
15 | TAN | 800 | Serial data
16 | BLK/WHT | 451 | PCM ground
17 | BLK | 2760 | IAT ground
18 |  |  | Not Used
19 | PNK | 439 | Ignition positive voltage
20 | ORN | 540 | Battery feed
21 |  |  | Not Used
22 | PNK | 1224 | Trans fluid pressure switch A input
23-27 |  |  | Not Used
28 | TAN/WHT | 1669 | HO2S sensor 2 signal low
29 | TAN | 413 | HO2S sensor 1 signal low
30 | PPL | 420 | TCC brake switch
31 | BLK | 2753 | Sensor ground
32 | GRY | 435 | GEGR valve control
33 | DK BLU | 496 | KS signal
34-35 |  |  | Not Used
36 | BRN | 25 | Charge warning indicator control
37 |  |  | Not Used
38 | LT GRN/WHT | 1749 | IAC B high
39-42 |  |  | Not Used
43 | BLK | 1744 | Injector number 1 control
44 | YEL/BLK | 1223 | 2-3 shift solenoid valve control
45 |  |  | Not Used
46 | PNK/BLK | 1746 | Injector number 3 control
47 | LT GRN/BLK | 1745 | Injector number 2 control
48 | RED/BLK | 453 | Reference low
49-52 |  |  | Not Used
53 | TAN/BLK | 424 | Bypass
54 | WHT | 423 | Ignition control (IC)
55 | DK GRN | 389 | Vehicle speed signal output
56 | BLK/WHT | 451 | PCM ground
57 | BLK/WHT | 451 | PCM ground
58 |  |  | Not Used
59 | PPL | 1807 | Class 2 data
60 | BLK/WHT | 451 | PCM ground
61 | BLK | 552 | TP ground
62 | DK BLU/WHT | 1231 | AT/ISS sensor low
63 | RED/BLK | 1230 | AT/ISS sensor high
64 | YEL | 400 | VSS high
65 | PPL | 401 | VSS low
66-67 |  |  | Not Used
68 | YEL | 772 | Transaxle range switch input B
69 | YEL | 492 | MAF sensor input
70 | DK BLU | 229 | Theft deterrent input
71 | ORN/BLK | 463 | Required torque
72 | DK GRN | 83 | Cruise disable output
73 | BLK/WHT | 845 | injector number 5 control
74 |  |  | Not Used
75 | DK GRN | 35 | Hot coolant indicator control
76 | DK GRN/WHT | 428 | EVAP canister purge valve control
77-78 |  |  | Not Used
79 | YEL/BLK | 846 | Injector Number 6 control
80 | BLK | 2751 | A/C pressure return

#### Power Control Module (PCM) C2

Connector Part Information |

• | 12191110

• | 80-Way F Metri-Pack 100 W Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 |  |  | Not Used
2 | WHT | 1310 | EVAP canister vent valve
3 | DK GRN/WHT | 465 | Fuel pump relay control
4 | RED | 1676 | EGR valve control
5 | BRN/WHT | 419 | MIL control
6 | BRN/WHT | 1173 | Low oil level indicator control
7 | LT BLU/WHT | 1747 | IAC A high
8 | WHT | 121 | Tachometer indicator control
9 | TAN/BLK | 464 | Delivered torque
10 | PPL | 412 | HO2S sensor 1 signal high
11 | PPL/WHT | 1668 | HO2S sensor 2 signal high
12-15 |  |  | Not Used
16 | WHT | 776 | Transaxle range Parity input
17 | RED | 1226 | Trans fluid pressure switch C input
18 | BLK/WHT | 771 | Transaxle range A input
19-21 |  |  | Not Used
22 | DK GRN/WHT | 762 | A/C request
23-24 |  |  | Not Used
25 | LT GRN | 432 | MAP sensor signal
26 | YEL | 410 | ECT sensor signal
27 | RED/BLK | 380 | A/C refrigerant pressure sensor signal
28 | BRN | 1456 | EGR solenoid position signal
29 |  |  | Not Used
30 | GRY | 2702 | 5 volt reference
31-32 |  |  | Not Used
33 | GRY | 2701 | 5 volt reference
34 | GRY | 2700 | 5 volt reference
35 | BLK | 2759 | Sensor ground
36-38 |  |  | Not Used
39 | DK GRN/WHT | 459 | A/C compressor clutch relay control
40-41 |  |  | Not Used
42 | LT BLU/BLK | 844 | Fuel Injection 4 control
43 |  |  | Not Used
44 | LT BLU/BLK | 1748 | IAC valve A low
45 | RED/BLK | 1228 | PC solenoid valve high
46 | LT BLU/WHT | 1229 | PC solenoid valve low
47-48 |  |  | Not Used
49 | LT GRN/BLK | 444 | IAC valve B low
50 | TAN | 472 | Intake air temperature sensor
51-54 |  |  | Not Used
55 | DK GRN | 890 | Fuel tank pressure sensor signal
56 | GRY | 773 | Transaxle range C input
57 | DK BLU | 1225 | Trans fluid pressure switch B input
58 | BRN | 1174 | Engine oil level indicator input
59 | WHT | 85 | Cruise status
60 |  |  | Not Used
61 | RED | 225 | Generator control
62 |  |  | Not Used
63 | PNK | 657 | TCC release switch input
64-65 |  |  | Not Used
66 | DK BLU | 417 | Throttle position sensor signal
67 |  |  | Not Used
68 | YEL/BLK | 1227 | Transaxle fluid temperature sensor
69 | PPL | 1589 | Fuel level sensor input
70 | LT GRN | 1867 | CMP/CKP sensor ground
71 |  |  | Not Used
72 | RED/WHT | 812 | CMP/CKP sensor battery positive voltage
73 | BLK | 407 | CMP/CKP sensor ground
74 | YEL/BLK | 1868 | CMP/CKP sensor battery positive voltage
75-77 |  |  | Not Used
78 | BRN | 418 | TCC PWM solenoid control
79-80 |  |  | Not Used

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 2701 | 5-volt reference A
B | BLK | 552 | TP ground
C | DK BLU | 417 | TP sensor signal

#### Transaxle Range Switch C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series Sealed (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 434 | PARK/NEUTRAL input
B | ORN | 840 | Fused battery feed
C | LT GRN | 275 | Transaxle range switch feed-PARK
D | BLK/WHT | 451 | PCM ground
E | PPL | 6 | Starter solenoid feed
F | LT GRN | 24 | Backup lamp feed
G | YEL | 5 | Ignition switched battery feed-START

#### Transaxle Range Switch C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transaxle range switch parity input
B | YEL | 772 | Transaxle range switch input B
C | GRY | 773 | Transaxle range switch input C
D | BLK/WHT | 771 | Transaxle range switch input A

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | VSS low
B | YEL | 400 | VSS high