For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Battery | Engine compartment, behind RH headlamp | -- | -- | --
Fusible Link A | Bolted to starter solenoid | -- | -- | --
Fusible Link Z | Bolted to starter solenoid | -- | -- | --
Fuse Block | RH side of I/P, in RF door opening | -- | -- | --
Generator (K68) | Top rear RH side of engine | -- | -- | --
Generator (KG9) | Top rear RH side of engine | -- | -- | --
Ignition Switch | Part of steering column | -- | -- | --
Instrument Cluster | LH side of I/P | -- | -- | --
Powertrain Control Module (PCM) | Engine compartment, secured in air cleaner assembly | -- | -- | --
Starter Motor | Lower front of engine | -- | -- | --
Starter Solenoid | Lower front of engine, part of starter motor assembly | -- | -- | --
Transaxle Range Switch | Rear LH side of engine compartment, mounted to top of transaxle | -- | -- | --
Underhood (UH) Electrical Center | Engine compartment, front of RH wheelhouse, above battery | -- | -- | --
C103 (2 cavities) | I/P wiring harness to engine wiring harness, in lower LH side of engine compartment, next to C101 | -- | -- | --
C201 (48 cavities) | I/P wiring harness to steering column wiring harness, mounted to LH side of steering column near base | -- | -- | --
G100 | Battery grounded to RH inner fender, near battery | -- | -- | --
G113 | Engine compartment, left of starter, along with battery ground | -- | -- | --
P100 | On RH side of bulkhead, left of RH strut tower | -- | -- | --
P101 | On LH side of bulkhead, right of LH strut tower | -- | -- | --
S209 | I/P harness, center of I/P approximately 8 cm (3 in) from security indicator lamp | -- | -- | --