For 1990-2009 cars

### Removal Procedure

1. Remove the driver's side instrument panel insulator retainers.
2. Remove the driver's side instrument panel insulator.
3. Cut the plastic tie strap securing the tape retract module to the wire harness.
4. Disconnect the tape retract module electrical connector.
5. Remove the tape retract module from the vehicle.

### Installation Procedure

1. Install the tape retract module to the vehicle.
2. Connect the tape retract module electrical connector.
3. Secure the tape retract module to the wire harness with a plastic tie strap.
4. Install the driver's side instrument panel insulator.
5. Install the driver's side instrument panel retainers.