For 1990-2009 cars

### Removal Procedure

1. Use a flat-bladed tool to remove the plastic center cap from the center of the recliner handle.
2. Grasp the recliner handle and pull it straight off the shaft.

### Installation Procedure

1. Install the recliner handle on the recliner shaft.
2. Push the recliner handle firmly onto the recliner shaft until fully seated.
3. Snap the plastic center cap into the center of the recliner handle.