For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for a poor connection or an open in circuit 389 between the driver information display harness connector terminal 9 and the Powertrain Control Module (PCM) harness connector C1 terminal 55. Is there an open or a poor connection? | -- | Go to Step 2 | Go to Step 3
2 | Repair the poor connection or the open in circuit 389 between the driver information display harness connector terminal 9 and the Powertrain Control Module (PCM) harness connector C1 terminal 55. Has the repair been made and the system rechecked? | -- | System OK | --
3 | Replace the driver information display. Refer to Driver Information Center Replacement . Has the repair been completed and the system rechecked? | -- | System OK | --