For 1990-2009 cars

# Warranty Admin. - June, 2000 Labor TIme Guide Updates

Subject: | June, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - A/B Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MANIFOLD AND/OR GASKET, INTAKE LOWER - R&R OR REPLACE

- POLICY E: (7/70 California - Includes other applicable states)

- NOTE: The 7/70 emission warranty applies only when the manifold and gasket are replaced as an assembly. The 7/70 emission warranty does not apply to gasket replace only.

R

J0224

4.7

- NOTE: Applies to Engine Code E

- ADD: A- To Replace Oil Pump Drive Seal

0.1

- B- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Necessary

0.3

*IND: N - New/R - Revised

#### LTG Update - C/K New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
SUPPORT, MECHANICAL LUMBAR - REPLACE |  |  |  |  |  |  |  |
PASSENGER | N | C7063 | -- | -- | -- | -- | 1.2 | 1.2
DRIVER | N | C7064 | -- | -- | -- | -- | 1.2 | 1.2

- ADD: A- With Side Impact Air Bag

--

--

--

--

0.4

0.4

HEATED SEAT COMPONENTS - REPLACE |  |  |  |  |  |  |  |
HEATING ELEMENT |  |  |  |  |  |  |  |
PASSENGER | N | C7170 | -- | -- | -- | -- | 0.9 | 0.9
HEATING ELEMENT |  |  |  |  |  |  |  |
DRIVER | N | C7171 | -- | -- | -- | -- | 0.9 | 0.9

- ADD: A- With Side Impact Air Bag

--

--

--

--

0.4

0.4

- B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

0-.03

0-.03

CASE, IGNITION LOCK CYLINDER (PASSLOCK) - REPLACE | R | E7202 | -- | -- | -- | 1.0 | 1.0 | 1.0
*IND: N - New/R - Revised

#### LTG Update - E/J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PUMP ASSEMBLY, FRONT AXLE AIR LOCK - REPLACE | N | F0026 | -- | -- | -- | 0.4 | 0.4 | 0.4

- ADD: A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

0-.03

0-.03

0-.03

*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PRE-DELIVERY INSPECTION - BASE TIME | R | Z7000 |  |  |  |  |  |
CHEVROLET |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4
PONTIAC |  |  | -- | -- | 1.4 | 1.4 | 1.4 | 1.4

- ADD: A- To Install Sunshade Package

--

--

0.1

0.1

0.1

0.1

- B- To Install NHRA Emblems Pontiac RPO 1SH

--

--

--

--

--

0.2

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CYLINDER, IGNITION LOCK - R&R OR REPLACE

- PART GP: 2.188

- INC. Disable and Enable SIR System.

R

E7200

1.1

1.3

1.3

1.3

0.5

0.5

- No Change to "ADD" Condition

MODULE, ANTENNA - REPLACE | N | R0520 | -- | -- | -- | -- | 0.4 | 0.4

- ADD: A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

0-.03

0-.03

*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MANIFOLD AND/OR GASKET, INTAKE LOWER - R&R OR REPLACE

- POLICY E: (7/70 California - Includes other applicable states)

- NOTE: The 7/70 emission warranty applies only when the manifold and gasket are replaced as an assembly. The 7/70 emission warranty does not apply to gasket replace only.

R

J0224

3.5

4.7

4.7

4.7

4.7

4.7

- NOTE: Applies to Engine Code D and E

- ADD: A- To Replace Oil Pump Drive Seal

0.1

0.1

0.1

0.1

0.1

0.1

- B- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Necessary

0.3

0.3

0.3

0.3

0.3

0.3

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MANIFOLD AND/OR GASKET, INTAKE - R&R OR REPLACE

- POLICY E: (7/70 California - Includes other applicable states)

- NOTE: The 7/70 emission warranty applies only when the manifold and gasket are replaced as an assembly. The 7/70 emission warranty does not apply to gasket replace only.

R

J0200

- NOTE: Applies to Engine Code D and E

EXC CHEVROLET |  |  | 3.5 | 3.5 | 3.5 | 3.5 | 3.5 | 3.5
CHEVROLET |  |  | 3.7 | 3.7 | 3.7 | 3.7 | 3.7 | 3.7

- ADD: A- To Replace Intake Manifold

0.3

0.3

0.3

0.3

0.3

0.3

- B- To Replace Oil Pump Drive Seal

0.1

0.1

0.1

0.1

0.1

0.1

- C- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Necessary

0.3

0.3

0.3

0.3

0.3

0.3

CANISTER, FUEL VAPOR - REPLACE

- PART GP: 3.130

- POLICY: E

R

L0620

CHEVROLET LUMINA |  |  | 0.3 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
CHEVROLET IMPALA & MONTE CARLO |  |  | 0.3 | 0.5 | 0.5 | 0.5 | 2.1 | 2.1
PONTIAC & OLDSMOBILE |  |  | 0.3 | 0.5 | 0.5 | 0.5 | 0.5 | 2.1
BUICK |  |  | 0.3 | 0.5 | 0.5 | 0.5 | 2.1 | 2.1
SENSOR, FUEL TANK VACUUM - REPLACE | R | L0622 |  |  |  |  |  |
CHEVROLET IMPALA |  |  | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.6
CHEVROLET LUMINA |  |  | -- | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
CHEVROLET MONTE CARLO |  |  | -- | 1.4 | 1.4 | 1.4 | 0.6 | 0.6
PONTIAC |  |  | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.6
OLDSMOBILE |  |  | -- | 1.4 | 0.2 | 0.2 | 0.2 | 0.6
BUICK |  |  | -- | 0.2 | 0.2 | 0.2 | 0.6 | 0.6
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

0-.03

0-.03

0-.03

0-.03

0-.03

NECK, FUEL TANK FILLER - REPLACE

- PART GP: 3.003

- POLICY: E

R

L1040

CHEVROLET LUMINA |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
CHEVROLET IMPALA & MONTE CARLO |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.2 | 0.2
PONTIAC & OLDSMOBILE |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.5 | 0.2
BUICK |  |  | 0.5 | 0.5 | 0.5 | 0.5 | 0.2 | 0.2
SEAL, FUEL SENDER/PUMP ASSEMBLY (TANK UNIT) - REPLACE

- POLICY: E

R

L1195

CHEVROLET LUMINA |  |  | 1.3 | 1.3 | 1.3 | 1.3 | 1.3 | 1.3
CHEVROLET IMPALA & MONTE CARLO |  |  | 1.3 | 1.3 | 1.3 | 1.3 | 0.9 | 0.9
PONTIAC |  |  | 1.3 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
OLDSMOBILE |  |  | 1.3 | 1.3 | 0.9 | 0.9 | 0.9 | 0.9
BUICK |  |  | 1.3 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9
SENSOR, FUEL LEVEL (TANK UNIT) - REPLACE | R | L1197 |  |  |  |  |  |
CHEVROLET LUMINA |  |  | -- | 1.5 | 1.5 | 1.5 | 1.5 | 1.5
CHEVROLET IMPALA & MONTE CARLO |  |  | -- | 1.5 | 1.5 | 1.5 | 1.0 | 1.0
PONTIAC |  |  | -- | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
OLDSMOBILE |  |  | -- | 1.4 | 1.0 | 1.0 | 1.0 | 1.0
BUICK |  |  | -- | 1.0 | 1.0 | 1.0 | 1.0 | 1.0
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

0-.03

0-.03

0-.03

0-.03

0-.03

SENDER AND/OR PUMP ASSEMBLY, FUEL (TANK UNIT) - REPLACE

- INC. R&R fuel tank and test gage.

- PART GP: 3.107

- NOTE: Also known as Fuel Module.

- NOTE: If replacing the "Fuel Vapor Pressure Sensor" use operation J6327.

R

L1200

CHEVROLET LUMINA |  |  | 1.3 | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
CHEVROLET IMPALA & MONTE CARLO |  |  | 1.3 | 1.4 | 1.4 | 1.4 | 0.9 | 0.9
PONTIAC |  |  | 1.3 | 0.7 | 0.7 | 0.7 | 0.7 | 0.7
OLDSMOBILE |  |  | 1.3 | 1.3 | 0.9 | 0.9 | 0.9 | 0.9
BUICK |  |  | 1.3 | 0.9 | 0.9 | 0.9 | 0.9 | 0.9

- NOTE: No Change to "ADD" Condition

TANK, FUEL - REPLACE

- PART GP: 3.001

- POLICY: E (7/70 California - Includes other applicable states)

R

L1260

CHEVROLET LUMINA |  |  | 1.3 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
CHEVROLET IMPALA & MONTE CARLO |  |  | 1.3 | 1.2 | 1.2 | 1.2 | 1.2 | 2.1
PONTIAC & OLDSMOBILE |  |  | 1.3 | 1.2 | 1.2 | 1.2 | 1.2 | 2.1
BUICK |  |  | 1.3 | 1.2 | 1.2 | 1.2 | 1.2 | 2.1
*IND: N - New/R - Revised