For 1990-2009 cars

## Rear SeatAudio Control Replacement VIN Code U

### Removal Procedure

1. Use a small flat-bladed tool in order to release the rear seat audio control tabs.
2. Remove the rear seat audio controls from the rear quarter trim.
3. Disconnect the electrical connectors.
4. Remove the rear seat audio controls from the rear quarter trim.

### Installation Procedure

1. Install the rear seat audio controls to the rear quarter trim.
2. Connect the electrical connectors.
3. Align the tabs on the rear seat audio controls to the slots in the rear quarter trim.
4. Press down on the rear sear audio controls in order to lock the tabs.

## Rear SeatAudio Control Replacement VIN Code X

### Removal Procedure

1. Use a small, flat-bladed tool in order to press on the locking tabs and release the rear seat audio controls from the rear overhead console.
2. Disconnect the electrical connectors.
3. Remove the rear seat audio controls from the rear overhead console.

### Installation Procedure

1. Connect the electrical connectors to the rear seat audio controls.
2. Align the rear seat audio controls to the rear overhead console.
3. Press the rear seat audio controls into the rear overhead console until fully seated and locked in.