For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief .
2. Drain the fuel tank. Refer to Fuel Tank Draining .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Note strainer (3) position for future reference.
6. Support the reservoir with one hand and grasp the strainer with the other hand.
7. Use a screwdriver to pry the strainer ferrule off the reservoir.
8. Discard the strainer.

### Installation Procedure

1. Install the new strainer to the reservoir.
2. Support the reservoir with one hand and grasp the strainer (4) with the other hand twisting the strainer into position.
3. Reinstall the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
4. Install the fuel tank. Refer to Fuel Tank Replacement .
5. Add fuel and reinstall the fuel fill cap.
6. Reconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in engine electrical.
7. Check for fuel leaks.

7.1. | Turn the ignition switch ON for 2 seconds.

7.2. | Turn the ignition switch OFF for 10 seconds.

7.3. | Turn the ignition switch ON.

7.4. | Check for fuel leaks.