General Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coil Spring Height-No Load | 265.5 ± 5 mm | 10.45 ± 0.02 in
Grease Type-Rear Wheel Bearing and Hub | M-8143 ANTIF BRG GREASE
Rear Wheel Bearing

- Clearance

0 mm

0 in

- No Load

0.137-0.422 N·m

1.2-3.7 lb in

Shock Absorber

- Maximum Length

444.8 ± 3 mm

17.51 ± 0.12 in

- Minimum Length

285.0 ± 3 mm

11.22 ± 0.12 in

- Stroke

160 mm

6.3 in