Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Control Arm Ball Joint Bolt | 50-70 N·m | 36-52 lb ft
Drive Axle Shaft Nut | 210 N·m | 155 lb ft
Oil Drain Plug | 25-30 N·m | 18-22 lb ft
Oil Level Plug | 36-54 N·m | 26-40 lb ft
Stabilizer Bar Bolt | 33-53 N·m | 24-39 lb ft
Stabilizer Bar Castellated Nut | 40-50 N·m | 30-36 lb ft
Tie Rod End Joint Castellated Nut | 30-55 N·m | 21-41 lb ft
Transaxle Under Cover Bolt | 35-55 N·m | 25-41 lb ft
Wheel Nut | 90-110 N·m | 66-81 lb ft