Lack of Power or Hesitation. Chevrolet Joy 2008

For 1990-2009 cars

#### Loss of Power

Checks | Actions
--- | ---
O/D switch | Faulty switch
ATF temperature sensor | Refer to DTC 17 .
Line pressure solenoid | Refer to DTC 48 .
Shift solenoid | Refer to DTC 53 and DTC 58 .
Transmission control module (TCM) | Refer to Diagnostic System Check - Automatic Transmission .
Oil pump | Damage or wear to the oil pump gears
Torque converter | Internal damage
Control valve spool sliding | Damage to the control valve spool
High clutch | Burn or wear of the high clutch. Refer to High Clutch Disassemble
2-4 brake band | Burnt or worn 2-4 brake band