Rear License Plate Lamp Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the license plate lamp screws.
3. Draw out the license plate lamp.
4. Remove the license plate lamp bulb.
5. Remove the license plate lamp from the tailgate handle.

### Installation Procedure

1. Install the license plate lamp bulb.
2. Install the license plate lamp.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the license lamp screws.
4. Connect the negative battery cable.