Disassembled Views. Chevrolet Joy 2008

For 1990-2009 cars

Figure 1:

#### Transmission Cut Away View

Figure 2:

#### Internal Components

(1) | Drive Plate Flange
(2) | Drive Plate
(3) | Rear Drive Plate
(4) | Torque Converter
(5) | Oil Pump Assembly
(6) | Input Shaft Assembly
(7) | Output Gear Assembly
(8) | Reduction Gear Assembly
(9) | Differential Assembly
(10) | Low and Reverse Brake Assembly
(11) | Low Clutch Assembly
(12) | Rear Internal Gear Assembly
(13) | Rear Planetary Carrier Assembly
(14) | Rear Sun Gear
(15) | Front Planetary Carrier Assembly
(16) | Front Sun Gear Assembly
(17) | Low One-Way Clutch Assembly
(18) | High Clutch Hub Assembly
(19) | High Clutch Assembly
(20) | Bearing
(21) | Seal Ring
(22) | Reverse Clutch Assembly
(23) | Bearing Race
(24) | Seal Ring
(25) | Washer
(26) | Anchor End Pin
(27) | Brake Band
(28) | Band Servo Piston Assembly

Figure 3:

#### Case and Associated Parts

(1) | Converter Housing
(2) | Transmission Case
(3) | Transmission Side Cover
(4) | Magnet
(5) | Oil Pan
(6) | Oil Level Gauge/Oil Filler Tube
(7) | Parking Lock Assembly
(8) | Manual Shaft Assembly
(9) | Park/Neutral Position (PNP) Switch
(10) | Control Valve Assembly
(11) | Solenoid Terminal
(12) | Vehicle Speed Sensor (VSS)
(13) | Oil Cooler
(14) | Input Shaft Speed (ISS) Sensor

Figure 4:

#### Oil Pump

(1) | Oil Pump Cover
(2) | Inner Rotor
(3) | Outer Rotor
(4) | Oil Pump Housing

Figure 5:

#### Reverse Clutch

(1) | Snap Ring
(2) | Retaining Plate
(3) | Reverse Clutch Plate
(4) | Friction Plates
(5) | Separator Plates
(6) | Snap Ring
(7) | Spring Retainer Assembly
(8) | Reverse Clutch Piston
(9) | O-Ring
(10) | Reverse Clutch Drum

Figure 6:

#### High Clutch

(1) | Spring Ring
(2) | Retaining Plate
(3) | High Clutch Plates
(4) | Friction Plates
(5) | Separator Plates
(6) | Spring Retainer
(7) | Snap Ring
(8) | Spring
(9) | High Clutch Piston
(10) | O-Ring
(11) | High Clutch Drum
(12) | Bearing
(13) | Seal Ring

Figure 7:

#### Low Clutch

(1) | Friction Plates
(2) | Separator Plates
(3) | Retaining Plates
(4) | Snap Ring
(5) | Low Clutch Plates
(6) | Cushion Plates
(7) | Spring Retainera
(8) | Spring
(9) | Cancel Cover
(10) | Low Clutch Piston
(11) | Low Clutch Drum
(12) | O-Ring

Figure 8:

#### First Reverse Brake

(1) | Separator Plates
(2) | Friction Plates
(3) | Retaining Plates
(4) | Snap Ring
(5) | Low and Reverse Brake Plates
(6) | Cushion Plate
(7) | Spring Retainer Assembly
(8) | Low and Reverse Brake Piston
(9) | O-Ring

Figure 9:

#### Control Valve Body

(1) | Upper Control Valve Body
(2) | Separator Plate A
(3) | Intermediate Control Valve Body
(4) | Separator Plate B
(5) | Lower Control Valve Body
(6) | Shift Solenoid B
(7) | Line Pressure Solenoid
(8) | Shift Solenoid A
(9) | Oil Strainer
(10) | Lock-Up Solenoid

Figure 10:

#### Upper Control Valve Body

(1) | Retainer Plate Pin
(2) | Spring
(3) | Neutral Shift Valve
(4) | Throttle Pressure Accumulator
(5) | Spring
(6) | Retainer Plate Pin
(7) | Retainer Plate Pin
(8) | Spring
(9) | Shift Valve A
(10) | Parallel Pin
(11) | Plug
(12) | Spring
(13) | Pressure Modifier Valve
(14) | Manual Valve
(15) | Retainer Plate Pin
(16) | Spring
(17) | Line Pressure Relief Valve

Figure 11:

#### Intermediate Control Valve Body

(1) | Retainer Plate Pin
(2) | Plug
(3) | Spring
(4) | 1-2 Modulator Valve
(5) | Retainer Plate Pin
(6) | Plug
(7) | Spring
(8) | Neutral Control Valve
(9) | Retainer Plate Pin
(10) | Valve Sleeve
(11) | Valve Plug
(12) | Spring
(13) | Lock-Up Control Valve
(14) | Retainer Plate Pin
(15) | Plug
(16) | Spring
(17) | Servo Release Timing Valve
(18) | Retainer Plate Pin
(19) | Spring
(20) | Shift Valve B
(21) | Retainer Plate Pin
(22) | Plug
(23) | Spring
(24) | Accumulator Control Valve
(25) | Retainer Plate Pin
(26) | Valve Sleeve
(27) | Valve Plug
(28) | Spring Seat
(29) | Spring
(30) | Pressure Regulator Valve
(31) | Retainer Plate Pin
(32) | Spring
(33) | Pilot Valve

Figure 12:

#### Lower Control Valve Body

(1) | Retainer Plate Pin
(2) | Spring
(3) | Torque Converter Relief Valve
(4) | Retainer Plate Pin
(5) | Plug
(6) | Spring
(7) | 1-2 Accumulator
(8) | Retainer Plate Pin
(9) | Plug
(10) | Spring Outer
(11) | Spring Inner
(12) | Throttle Pressure Accumulator
(13) | Retainer Plate Pin
(14) | Plug
(15) | Spring Outer
(16) | Spring Inner
(17) | Low Clutch Accumulator

Figure 13:

#### Control Valve Body Bolt Installation Position

(1) | Shift Solenoid A
(2) | Lock Up Solenoid
(3) | Line Pressure Solenoid
(4) | Shift Solenoid B

Bolt | Bolt Length (mm) | Bolt Length (in)
--- | --- | ---
A | 20 | 0.8
B | 77 | 3.0
C | 12 | 0.5
D | 87 | 3.4
E | 90 | 3.5
Important: All bolts are torqued to 8 N·m (70 lb in).