Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter Heat Shield | 8-12 N·m | 71-106 lb in
Front Exhaust Pipe-to-Exhaust Manifold Nuts | 25-35 N·m | 18-25 lb ft
Front Exhaust Pipe-to-Front Muffler Pipe Nuts | 25-35 N·m | 18-25 lb ft
Front Exhaust Pipe-to-Pup-up Catalytic Converter | 25-35 N·m | 18-25 lb ft
Front Muffler-to-Rear Muffler nuts | 25-35 N·m | 18-25 lb ft
Muffler Clamp Nut | 24-28 N·m | 18-21 lb ft
Pup-up Catalytic Convertor-to-Exhaust Manifold Bolt | 25-35 N·m | 18-25 lb ft
Rear Muffler Heat Shield | 8-12 N·m | 71-106 lb in