Fastener Tightening Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Heater | 60 N·m | 44 lb ft
Coolant Pipe Bolt | 8-15 N·m | 71-130 lb in
Coolant Pump Bolt/Nut | 9-12 N·m | 80-106 lb in
Coolant Pump Stud Bolt | 9-12 N·m | 80-106 lb in
Coolant Temperature Sensor | 20 N·m | 15 lb ft
Distributor Case Bolt/Nut | 8-12 N·m | 71-106 lb in
Electric Cooling Fan Assembly Bolt | 3.5-4.5 N·m | 31-40 lb in
Electric Cooling Fan Motor Nut | 3.0-3.2 N·m | 27-28 lb in
Engine Coolant Temperature Sensor | 10 N·m | 89 lb in
Radiator Mounting Bracket Bolt | 3.5-4.5 N·m | 31-40 lb in
Thermostat Housing Bolt | 8-15 N·m | 71-130 lb in
Water Inlet Cap Bolt | 8-12 N·m | 71-106 lb in