RPO Code List. Chevrolet Joy 2008

For 1990-2009 cars

RPO | Description
--- | ---
11U | Body Color - Galaxy White
12U | Body Color - Ocean Blue
23U | Body Color - Jazz Blue
45U | Body Color - Apple Green
52U | Body Color - Highway Yellow
56U | Body Color - Electric Yellow
5MB | Load Compartment Trim - Side Trim - Luggage Room, Plastic
5MC | Load Compartment Trim - RR Side Load Compartment
71U | Body Color - Super Red
82I | Interior Key Color - Tar Grey
87U | Body Color - Pearl Black
92U | Body Color - Poly Silver
98U | Body Color - Dynamic Orange
99U | Body Color - Mighty Blue
A03 | Glass - Tinted Glass and Windshield Top Band
A32 | Window Regulator - Front Only Power
A50 | Front Seat - Standard
A51 | Front Seat - Custom
A60 | Tail Gate Opening - Key Type, Manual
A70 | Seat Belt - Front, 3 Point ELR w/Pretensioner
A91 | Tail Gate Opening - Remote Release
AAM | Knee Protector - Driver
AE3 | Window Regulator - All Power
AH9 | Front Seat - Height Adjust - Driver
AIA | Seat Belt - Front, 3 Point ELR - Co-Driver Side
AIF | Seat Belt - Front, 3 Point ELR w/Load Limiter - Driver Side
AIG | Seat Belt - Front, 3 Point ELR - Driver Side
AJ3 | Single Air Bag
AJ7 | Dual and Side Air Bag
AK5 | Dual Air Bag
AKA | Glass - Clear Glass
AM4 | Rear Seat - Split Collapsible w/Headrest (3EA)
AM7 | Rear Seat - One Piece Folding
AM9 | Rear Seat - Split Collapsible w/o Headrest
APW | Window Regulator - All Manual
AQ2 | Trunk Net
AQ4 | Rear Seat - Split Collapsible w/Headrest (2EA)
AR1 | Air Bag - Delete
AT3 | Child Seat Tether Anchorage Provision
AT7 | Seat Belt - Rear, 3 Point L/R and Center Belt - ELR
AU3 | Central Door Lock
AWB | Seat Belt - Rear, 3 Point L/R and 2 Point Center Lap Belt - ELR
B00 | Indonesia - Mandatory (Dual Reverse Light)
B02 | South Africa - Mandatory (Non Reflective Rear Dummy Lens)
B04 | Equipment Additional Taiwan
B09 | Egypt - Mandatory
B12 | Russia - Mandatory
B6E | Molding - Rocker, Sporty
B79 | Meter Cluster Color - Blue
B7S | Parcel Shelf w/String, Rear
BAE | Engine Immobilizer
BLQ | I.D Plate - Type "A"
BLS | I.D Plate - Type "B"
BLV | I.D Plate - Type "D"
BLW | I.D Plate - Type "E"
BMC | I.D Plate - Type "H-1"
BMF | Badge - Pontiac
BMG | Badge - Daewoo
BMS | I.D Plate - Delete
BPZ | I.D Plate - Type "T"
BW2 | Wide Body Side Molding
BXB | Door Trim - Formed Type - Part Fabric
BXM | Door Trim - Formed Type - Plastic
C13 | Windshield Wiper and Washer - 2 Speed W/Intermittent
C1V | Metallic Paint
C25 | RR Window Wiper and Washer
C3Z | RR Window Defogger, w/o Timer
C46 | Heater
C60 | Manual Air Conditioner
C66 | Uncompleted Air-Con
CCB | Sun Roof, Manual Tilting
CK1 | Pakistan - Mandatory
CK2 | Yemen
CR8 | Egypt
CR9 | Morocco
CS1 | Tunisia
CS2 | Nigeria
CS5 | Angola
CS6 | Ethiopia
CU7 | Kuwait
CU8 | Saudi Arabia
CV4 | Israel
CV8 | Iraq
CX8 | Syria
CX9 | Lebanon
CY2 | Jordan
CY3 | Cameroon
CY4 | Ivory Coast
CY6 | Gabon
D1S | Meter Cluster Color - Orange
D2G | Algeria
D2J | Guinea
D2K | Grenada
D2L | St Lucia
D2O | Curacao
D2U | Guyana
D2Y | Antigua
D31 | Inside Rear View Mirror - Day and Night
D3B | Bermuda
D3D | Trinidad
D3E | Eritrea
D3G | Cape Verde
D3I | Barbados
D3J | Cayman Islands
D3K | Dominican Republic
D3L | El Salvador
D3M | Guatemala
D3P | Haiti
D3Q | Honduras
D3R | Jamaica
D3S | Qatar
D3U | St Maarten
D4C | Bahrain
D4G | Bahamas
D4H | Belize
D4N | Costa Rica
D4X | Aruba
D5D | Nicaragua
D5F | Senegal
D5K | Surinam
D5P | U.A.E
D63 | Front Seat - Seat Under Tray, Co-DR
D6F | Congo
D6J | Sun Visor - Driver - w/o Vanity Mirror + Codriver - w/Vanity Mirror & Cover
D72 | Outside Door Handle - Molded Color
D75 | Outside Door Handle - Body Color
D80 | Rear Spoiler - Body Color
D87 | Tailgate Handle Cover - Molded Color
D91 | Tailgate Handle Cover - Body Color
DBI | OSRVM, Foldable - Glass Moving Type
DD2 | Sun Visor - Driver - w/Vanity Mirror and Cover + Codriver - w/Vanity Mirror and Cover
DG2 | OSRVM, Foldable - Internal Adjustable
DHG | Sun Visor - Driver - w/o Vanity Mirror + Codriver - w/o Vanity Mirror
DHH | Sun Visor - Driver - w/Vanity Mirror & Cover + Codriver - w/o Vanity Mirror
DL6 | OSRVM, Foldable - Elec/Cont, MAN/FLDG (Both Side)
DLB | Floor Covering - Carpet w/Driver Side Heel Pad
DNB | OSRVM, Foldable - Elec. Adjustable (Co-DrIver Side)
DP5 | OSRVM, Foldable - Molded Color
DQ9 | OSRVM, Foldable - Body Color
DT4 | Ashtray - Detachable, w/o Lamp
DVG | Meter Cluster Color - Green
E11 | Mexico - Mandatory (Dual Reverse Light)
E12 | Japan - Mandatory (For Parallel Import Only, Dual Reverse Light)
E17 | Bumper 2.5 MPH
E22 | Assist Grip - RR Both Side (Dri.Side: w/Coat Hook, Co-Dri.Side: w/o Coat Hook)
E27 | Assist Grip - Co-Driver Side
E2U | Lettering - Trim Level - LS
E6G | Ghana
E6H | Oman
E7B | Liberia
E7C | Libya
E7E | Madagascar
E7J | Mauritius
E7Q | British Virgin Is.
E7W | Fire Extinguisher 0.5 kg
E87 | Wheel Trim - Styled Standard
E91 | Front Seat - Seatback Pocket (Co-Driver Side)
EF2 | Guinea - Bissau
EF5 | Panama
ELH | Front Seat - Side Pocket, Co-Driver
ERI | Battery Saver
F77 | Ratio Transaxle Final Drive 4.11
F81 | Ratio Transaxle Final Drive 4.71
FRI | Ratio Transaxle Final Drive 4.26
FWL | Ratio Transaxle Final Drive 4.44
GFM | Equipment Regional General Countries
GFS | Equipment Regional Gulf
J41 | Brake - FRT, DISC, RR, Drum
JM4 | Brake System PWR, FRT DISC, RR Drum, Cast Iron, Antilock, FRT and RR WHL
K11 | Air Filter
K35 | Special Area Package - High Altitude
K36 | Special Area Package - Low Volatility Fuel
K91 | Alternator - 65A
KE1 | Chile - Mandatory (Dual Reverse Light)
KIM | Trim Level - SE
KIX | Trim Level - SX
KRB | Fuel Rating Octane No. 83
KRC | Fuel Rating Octane No. 87
KRD | Fuel Rating Octane No. 91
KRE | Fuel Rating Octane No. 95
L11 | 1.0 SOHC MPI
LBF | 0.8 SOHC MPI
LHD | Left - Hand Drive
MFG | Transmission, Manual - Y4M, 5 Speed
MFL | Transmission, Automatic T/M, 4 Speed
MXG | Transmission, Manual - Y4A, 5 Speed
N12 | Exhaust Muffler - Standard
N27 | Steering Wheel 2 Spokes, STD
N40 | Steering - Power
N45 | Steering Wheel 3 Spokes
N51 | Steering - Manual
NPH | Exhaust Muffler - Heavy Duty
NQP | Unleaded - US83
NQT | Leaded - ECE 83
NT2 | EURO Stage II
NT3 | EC2000
NT4 | EC2005
P34 | Spare Wheel and Tire - Regular
PA6 | Wheel 13 X 4.5J, Steel - Styled
PB0 | Wheel Trim - Flush Wheel Cover - 13
PY5 | Wheel 13 X 4.5J, Steel
PZH | Wheel 13 X 4.5J, Alloy
QDY | 155/65 R13 Tire
QDZ | 145/70 R13 Tire
QI0 | Trim Level - #0
QI1 | Trim Level - #1
QI2 | Trim Level - #2
QQ6 | Spare Wheel and Tire - Temporary
QVH | 155/70 R13 Tire
RHD | Right - Hand Drive
T2C | Special Area Package - Cold Area
T2Y | Rear Seat - ISOFIX Child Seat Provision (Lower Anchorage)
T44 | Speed Warning - 120 km/h
T61 | Day Time Running Light
T79 | Fog Lamp, Rear
T84 | Head Lamp - ECE - Regulation, LHD
T85 | Head Lamp - ECE - Regulation, RHD
T89 | Rear Combi Lamp - ECE
T90 | Side Indicator - Fender
T96 | Front Fog Lamp
TB9 | Battery 35 AH
TDW | Coating Steel For BIW - Body PNL - Widen Area Coating
TDX | Lettering - Company Name - Daewoo
TDY | Lettering - Company Name - Chevrolet
TH5 | Seat Belt Height Adjust - Front, Driver
TP4 | Battery 45 AH
TR6 | Head Lamp - Leveling Device
TS6 | CHMSL
U17 | Instrument Cluster - w/o Tachometer
U18 | Instrument Cluster - Kilometers
U25 | Luggage Room Lamp
U2D | Instrument Cluster - w/ Tachometer
U37 | Cigar Lighter - w/o Lamp
U71 | Antenna - Roof, Front Center
UA5 | Theft Deterrent Sys Passive, Keyless Entry/Security
UAD | Speaker, FRT - STD (2EA)
UAK | Audio - S/DIN - 40Wx4Ch, Logic/CDP/RDS
UAL | Audio - RDS
UC1 | Instrument Cluster - Miles
UE8 | Instrument Cluster - Digital Clock
UK5 | Audio - S/DIN - 7Wx4Ch, Mech
UPK | Audio - S/DIN - 40Wx4Ch, LOGIC/CDP/MP3/RDS
UPR | Audio - D/DIN - 45Wx4Ch, TAPE/CDP/W/MP3
UPZ | Audio - S/DIN - 25Wx4Ch, MECH
UQ4 | Speaker - 4EA (Front and Rear)
UW6 | Speaker - 6EA (Front and Rear and Tweeter)
V54 | Roof Rack
VA8 | Label - Spanish
VD0 | Card Holder
VEE | Bumper Color - Body Color
VEJ | Bumper Color - Two Tone
VFT | Coating Steel For BIW - Body PNL - Basic Area Coating
VH4 | Mud Guard
VIX | VIN - Visual
VIY | Asterisk(*) Mark
VK8 | Sunglass Holder
VMB | Bumper Color - Molded Color
VNR | VIN Model Year 2007
VNS | VIN Model Year 2008
VNT | VIN Model Year 2009
VNU | I.D Body - US Type
VNW | I.D Body - EU (ISO) Type
VR2 | Trailer Connection Provision (Dealer Option)
W2V | Lettering - Company Name - Delete
W4U | Seat Covering - Full Cloth - DLX2
W6C | Seat Covering - Full Cloth - STD
W6E | Seat Covering - Full Cloth - DLX1
W6G | Seat Covering - Full Cloth - DLX4
W6H | Seat Covering - Full Cloth - DLX3
WAM | Lettering - Car Name (Matiz)
WAS | Lettering - Car Name (Spark)
WCM | Lettering - Trim Level - LT
WU5 | Dimmer - Inst. Cluster
XA6 | ECE Label
XN2 | Wheel Trim - Styled Deluxe
XX7 | Audio - Blank Cover w/Audio Wiring Harness
XZ1 | Special Area Package - Hot Area
Y9Y | Badge - Chevrolet