Harsh Park or Neutral to Drive Engagement. Chevrolet Joy 2008

For 1990-2009 cars

Checks | Causes
--- | ---
ATF temperature sensor | Refer to DTC 17
Line pressure solenoid | Refer to DTC 48
Shift switch positioning | Refer to Park/Neutral Position Switch Replacement
Transmission control module (TCM) | Refer to Diagnostic System Check - Automatic Transmission .
Low clutch | Burn or wear of the low clutch. Refer to Low Clutch Disassemble
Low clutch accumulator | Malfunction of accumulator
Broken or damaged oil pump | Seized or broken pump gears
Control valve spool | Control valve spool error