No Torque Converter Clutch Apply. Chevrolet Joy 2008

For 1990-2009 cars

#### No Torque Converter Clutch (TCC) Apply

Checks | Causes
--- | ---
Lock-up solenoid | Refer to DTC 43 .
Engine speed sensor | Refer to DTC 22 .
ATF temperature sensor | Refer to DTC 17 .
Vehicle speed sensor | Refer to DTC 22 .
Turbine sensor | Refer ti DTC 15 .
Shift switch | Refer to DTC 55 .
Transmission control module (TCM) | Refer to Diagnostic System Check - Automatic Transmission .
Control valve spool | Control valve spool error
Torque converter | Internal failure