Front Floor Console Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the floor console center screws.
2. Remove the gear shift lever boot cover.
3. Remove the floor console rear screws.
4. Remove the floor console.

### Installation Procedure

1. Install the floor console.
2. Install the floor console rear screws.
3. Install the gear shift lever boot cover to the floor console.
4. Install the floor console front screws.