Radio Antenna Module Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
3. Remove the antenna screw from inside the vehicle (2).
4. Remove the roof antenna (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the roof antenna with the screw (1).

Tighten
Tighten the roof antenna retaining screw to 3 N·m (27 lb in).

2. Install the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
3. Connect the negative battery cable.