ABS Component Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antilock Brake System (ABS) Main Relay Operation Voltage | 10.3-14.5 V
Antilock Brake System (ABS) Type | 4 Channel 4 Sensor
Speed Ring

- Inside Diameter - Front

65 mm

2.5590 in

- Inside Diameter - Rear

58 mm

2.2835 in

- Outside Diameter - Front

75.8 mm

2.9842 in

- Outside Diameter - Rear

69 mm

2.7165 in

- Tooth Volume of the Speed Ring

40 EA

Wheel Speed Sensor - Resistance | 1,000-1,500 Ω