Tire Diagnosis - Irregular or Premature Wear. Chevrolet Joy 2008

For 1990-2009 cars

1. Measure the depth of the tire tread.
2. Indicators appear when the tire tread depth becomes shallow, less than the depth of the tread wear indicator (a).

Specification
The depth of the tread wear indicator is 1.6 mm (0.06 in).

3. If the depth of the tread is below the specified value, replace the tire.

#### Tire Wear

(1) | Under-Inflation, Hard Cornering, Lack of Regular Rotation
(2) | Incorrect Wheel Alignment, Hard Cornering, Lack of Regular Rotation
(3) | Incorrect Wheel Alignment
(4) | Over-Inflation, Heavy Acceleration, Lack of Regular Rotation
(5) | Normal Wear to the Wear Indicator