Sunroof Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof screen clips (2).
2. Remove the sunroof screen lock (3).
3. Remove the sunroof screen (1).
4. Remove the inside sunroof molding (1) in the passenger compartment.
5. Remove the lower sunroof frame screws (2).
6. Remove the lower sunroof frame (1).
7. Remove the upper sunroof frame (1).

### Installation Procedure

Important: When installing the lower sunroof frame, make sure to tighten the screws previously as shown in the figure and tighten all the screws.

1. Install the upper sunroof frame.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the lower sunroof frame with the screws (1).

Tighten
Tighten the screws to 3 N·m (27 lb in).

3. Install the inside sunroof molding.
4. Install the screen with the clips and the lock.