General Specifications. Chevrolet Joy 2008

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coil Spring Height - No Load | 352 mm | 13.86 in
Grease Type - Front Wheel Bearing and Hub | M-8143 ANTIF BRG GREASE
Shock Absorber

- Maximum Length

465-471 mm

18.3-18.54 in

- Minimum Length

324-327 mm

12.76-12.87 in

- Stroke

144 mm

5.67 in

Stabilizer Shaft Diameter | 22 mm | 0.87 in
Suspension Type | Mcpherson Strut