Center Pillar Lower Trim Panel Replacement. Chevrolet Joy 2008

For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (1) on the lower center pillar trim panel.
2. Remove the spacer and the spring washer (2).
3. Remove the plastic protector from the seat belt anchor.
4. Pry off the lower center pillar trim panel.

### Installation Procedure

1. Install the lower center pillar trim panel.
2. Install the bolt on the lower center pillar trim panel. Refer to Front Seat Belt Replacement .