Lubrication Specifications. Chevrolet Joy 2008

For 1990-2009 cars

## Lubrication Specifications 0.8L

Application | Specification
--- | ---
Metric | English
Grease Capacity

- Inner

90-100 g

3.2-3.5 oz

- Outer

80-90 g

2.8-3.2 oz

Length

- Right

553.5 mm

21.79 in

- Left

386.5 mm

15.22 in

Shaft Diameter | 22 mm | 0.87 in
Type

- Inner

Tripot Joint

- Outer

Rzeppa Joint

## Lubrication Specifications 1.0L

Application | Specification
--- | ---
Metric | English
Grease Capacity

- Inner

90-100 g

3.2-3.5 oz

- Outer

80-90 g

2.8-3.2 oz

Length

- Right

607.5 mm

23.9 in

- Left

339 mm

13.3 in

Shaft Diameter | 22 mm | 0.87 in
Type

- Inner

Tripot Joint

- Outer

Rzeppa Joint