Control Solenoid Valve and Transmission Control Module Assembly Installation. Chevrolet Nubira (Delta) 2010

For 1990-2009 cars

Callout | Component Name
--- | ---

1

Control Solenoid Valve Assembly Filter Plate

Caution: Use care when removing or installing the filter plate assembly. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

Tip
Install a NEW filter plate to prevent fluid leaks past the fluid seals.

2 | Control Solenoid (w/Body and TCM) Valve Assembly
3 | Control Valve Body Bolt M5 x 40.5 (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
4 | Control Valve Body Bolt M6 x 97 (Qty: 12) Tighten 12 N·m (106 lb in)