ABS Components. GMC Truck Export Savana 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
Brake Pressure Differential Switch | Part of electronic brake control module, LH frame rail near center of vehicle | Component Location Views in Electrical Diagnosis | Antilock Brake System Connector End Views | --
Cruise Control Module | Front of engine compartment, near LH fender | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Data Link Connector (DLC) | Under LH side of IP | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Daytime Running Lamps Control Module | Under LH side of IP, taped on IP harness | Antilock Brake System Component Views | Connector End Views in Electrical Diagnosis | --
Electronic Brake Control Lamp Relay | Underhood fuse-relay center, LH front of engine compartment | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Electronic Brake Control Module (EBCM) | LH frame rail, near center of vehicle | Antilock Brake System Component Views | Antilock Brake System Connector End Views | --
EVO/Passlock Module | IP carrier, right of steering lolumn | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Instrument Cluster | Top LH side of IP | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
IP Fuse Block | LH lower kick panel | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Powertrain Control Module (PCM) | Under Center of IP | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
TCC/Stoplamp Switch | Under brake pedal | Component Location Views in Electrical Diagnosis | Antilock Brake System Connector End Views | --
Underhood Fuse-Relay Center | Engine compartment, LH fender | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Vehicle Control Module (VCM) | Engine compartment, LH fender | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Vehicle Speed Sensor (VSS) | LH side of transmission | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
Vehicle Speed Sensor Buffer | Below LH side of IP, near steering column | Component Location Views in Electrical Diagnosis | Antilock Brake System Connector End Views | --
Wheel Speed Sensor, LF | At LF wheel | Antilock Brake System Component Views | Antilock Brake System Connector End Views | --
Wheel Speed Sensor, RF | At RF wheel | Antilock Brake System Component Views | Antilock Brake System Connector End Views | --
C100 | LH rear of engine compartment at bulk | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
D103 (4.3L, 5.0L) | Engine harness, approx 20.0 cm from Underhood Fuse Relay Center | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
D103 (6.5L) | Engine harness, approx 10.0 cm from Splice 153 | Component Location Views in Electrical Diagnosis | Connector End Views in Electrical Diagnosis | --
G101 | Engine harness, near thermostat housing | Component Location Views in Electrical Diagnosis | -- | --
G102 | Engine harness, near generator bracket | Component Location Views in Electrical Diagnosis | -- | --
G102 (6.5L) | LH front of engine harness, at generator bracket, near A/C compressor | Component Location Views in Electrical Diagnosis | -- | --
G103 (4.3L) | Engine harness, at generator bracket | Component Location Views in Electrical Diagnosis | -- | --
G103 (5.0L, 5.7L, 7.4L) | LH front of engine harness, at generator bracket, near A/C compressor | Component Location Views in Electrical Diagnosis | -- | --
G103 (6.5L) | Engine harness, at generator bracket | Component Location Views in Electrical Diagnosis | -- | --
S101 (4.3L) | Engine harness, approx 20 cm from knock sensor breakout toward EBCM | -- | -- | --
S101 (5.0L, 5.7L) | Engine harness, approx 10 cm from ignition coil breakout toward fuel injector breakout | -- | -- | --
S101 (7.4L) | Engine harness, approx 5 cm from generator breakout toward C107 breakout | -- | -- | --
S101(6.5L) | Engine harness, approx 22 cm from optical fuel temperature sensor breakout toward C100 breakout | -- | -- | --
S102 (4.3L) | Engine harness, approx 104 cm from underhood fuse-relay center toward A/C compressor breakout | -- | -- | --
S102 (5.0L, 5.7L) | Engine harness, approx 4 cm from A/C compressor breakout toward MAF sensor breakout | -- | -- | --
S102 (7.4L) | Engine harness, approx 4 cm from main harness that leads to the A/C compressor breakout toward generator breakout | -- | -- | --
S102 (6.5L) | Engine harness, approx 4 cm from main harness that leads to the blower motor breakout toward C100 breakout | -- | -- | --
S103 (7.4L) | Engine harness, approx 4 cm from ECT sensor breakout toward C100 | -- | -- | --
S111 | Engine harness, approx 4 cm from main harness breakout that leads to the underhood fuse-relay center and C100 breakouts | - | -- | --
S122 (4.3L) | Engine harness, approx 7 cm from G103 breakout toward transmission | -- | -- | --
S122 (5.0L, 5.7L) | Engine harness, approx 24 cm from A/C compressor breakout toward C100 | -- | -- | --
S122 (7.4L) | Engine harness, approx 8 cm from C100 breakout toward VCM breakout | -- | -- | --
S152 (4.3L) | Engine harness, approx 16 cm from fuel injector breakout toward G103 breakout | -- | -- | --
S152 (5.0L, 5.7L) | Engine harness, approx 4 cm from fuel injector breakout toward G103 breakout | -- | -- | --
S153 (4.3L) | Engine harness, approx 4 cm from the A/C compressor breakout toward transmission | -- | -- | --
S153 (5.0L, 5.7L) | Engine harness, approx 8 cm from ignition coil breakout toward transmission | -- | -- | --
S153 (7.4L) | Engine harness, approx 4 cm from C100 breakout toward EGR sensor breakout | -- | -- | --
S153 (6.5L) | Engine harness, approx 27 cm from main harness breakout that leads to the underhood fuse-relay center | -- | -- | --
S154 (4.3L) | Engine harness, approx 98 cm from underhood fuse-relay center toward A/C compressor breakout | -- | -- | --
S154 (5.0L, 5.7L) | Engine harness, approx 4 cm from the ignition coil breakout toward the transmission | -- | -- | --
S154 (7.4L) | Engine harness, approx 3 cm from MAF sensor breakout toward the ECT sensor breakout | -- | -- | --
S156 (4.3L) | Engine harness, approx 14 cm from the knock sensor breakout toward the EBCM | -- | -- | --
S156 (5.0L, 5.7L) | Engine harness, approx 8 cm from the fuel injector harness breakout toward the ignition coil breakout | -- | -- | --
S156 (7.4L) | Engine harness, approx 10 cm from A/T ISS sensor breakout toward the fuel injector harness breakout | -- | -- | --
S156 (6.5L) | Engine harness, approx 4 cm from the brake pressure differential switch breakout toward transmission | -- | -- | --
S207 | IP harness, approx 4 cm into VSSB breakout | -- | -- | --
S210 | IP harness, approx 4 cm into TCC/Stoplamp switch breakout | -- | -- | --
S216 | IP harness, approx 8 cm from C200 breakout toward instrument cluster breakout | -- | -- | --
S231 | IP harness, approx 18 cm from C100 breakout toward park brake warning switch breakout | -- | -- | --