SMU - SECTION 10-A - TOP TETHER ANCHOR. GMC Truck Export Savana 1997

For 1990-2009 cars

# SMU - SECTION 10-A - TOP TETHER ANCHOR

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 10-A - TOP TETHER ANCHOR

#### MODELS: 1996-97 CHEVROLET AND GMC G MODELS

THIS BULLETIN REVISES THE TOP TETHER INSTALLATION ON PAGE 10A2-14 IN THE 1997 G VAN SERVICE MANUAL BY INCLUDING HARDWARE TO BE USED. THE SAME INSTRUCTIONS AND HARDWARE CAN ALSO BE USED FOR THE 1996 G VAN. FOR G VAN TOP TETHER HARDWARE, USE THE FOLLOWING COMPONENTS FROM THE C/H CAR ANCHOR KIT 25606689. INSTALL THE COMPONENTS AS INDICATED IN THE SERVICE MANUAL.

FIGURES: 0 ATTACHMENTS: 2

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1997 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.